**ΠΡΟΔΙΑΓΡΑΦΗ ΕΝΟΠΛΩΝ ΔΥΝΑΜΕΩΝ**

ΤΡΟΠΟΠΟΙΗΣΗ 1η

ΠΕΔ – Α – 01275 2ης ΕΚΔΟΣΗΣ

**«ΕΝ ΣΥΝΕΧΕΙΑ ΥΠΟΣΤΗΡΙΞΗ (ΕΣΥ)**

**ΤΑΧΥΠΛΟΩΝ ΣΚΑΦΩΝ ΜΕΤΑΦΟΡΑΣ ΠΡΟΣΩΠΙΚΟΥ**

**ΤΥΠΟΥ VIKING NORSAFE MUNIN S-1200»**

ΧΧ ΙΟΥΝΙΟΣ 2025

ΕΛΛΗΝΙΚΗ ΔΗΜΟΚΡΑΤΙΑ

ΥΠΟΥΡΓΕΙΟ ΕΘΝΙΚΗΣ ΑΜΥΝΑΣ

|  |  |
| --- | --- |
|  | |
| ΑΔΙΑΒΑΘΜΗΤΟ – ΑΝΑΡΤΗΤΕΟ  ΣΤΟ ΔΙΑΔΙΚΤΥΟ | |  | |

**3. ΤΑΞΙΝΟΜΗΣΗ**

Κωδικοί CPV (Common Procurement Vocabulary) και ACodP-2/3 (Allied Codification Publication)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Α/Α** | **ΓΕΝΙΚΗ ΠΕΡΙΓΡΑΦΗ ΥΛΙΚΟΥ** | **CPV** | **ACodP-2/3** | **ΠΑΡΣΕΙΣ** |
| 1 | Κήτη και μηχανικά ανταλλακτικά για πολεμικά πλοία | 35521000-2 | 2010 |  |
| 2 | Κινητήρες και μέρη κινητήρων για πολεμικά πλοία | 35521100-3 | 2850 |  |
| 3 | Ηλεκτρονικά και ηλεκτρικά ανταλλακτικά για πολεμικά πλοία | 35522000-9 | 2010 |  |
| 4 | Ανταλλακτικά και εξαρτήματα ραντάρ | 32352200-7 | 5840 |  |
| 5 | Διάφορα ανταλλακτικά | 34913000-0 | 2010 |  |
| 6 | Μέρη εξοπλισμού ραδιοεπικοινω-νίας και ραντάρ | 32352100-6 | 5840 |  |
| 7 | Ανταλλακτικά και εξαρτήματα ραντάρ | 32352200-7 | 5840 |  |
| 8 | Συγκροτήματα ραντάρ | 34932000-9 | 5840 |  |
| 9 | Συσκευές ραδιοεντοπισμού (ραντάρ) | 35722000-1 | 5840 |  |
| 10 | Συσκευές ραντάρ | 38115000-4 | 5840 |  |
| 11 | Συστήματα παγκόσμιας πλοήγησης και παγκόσμιου προσδιορισμού θέσης (GPS ή ισοδύναμα) | 38112100-4 | 5825 |  |
| 12 | Όργανα πλοήγησης και μετεωρολογίας | 38100000-6 | 6660 |  |
| 13 | Όργανα ναυσιπλοΐας | 38110000-9 | 6605 |  |
| 14 | Εξοπλισμός προσανατολισμού | 38111000-6 | 6605 |  |
| 15 | Πυξίδες | 38111100-7 | 6605 |  |
| 16 | Συσκευές ηχητικού εντοπισμού | 38113000-0 | 5845 |  |
| 17 | Συσκευές ραδιοβόλισης | 38124000-0 | 5860 |  |
| 18 | Κάμερες Ιστού | 30237240-3 |  |  |
| 19 | Υπηρεσίες αναβάθμισης επισκευής και συντήρησης πλοίων | 50241000-6 | 2040 |  |

**4. ΤΕΧΝΙΚΑ ΧΑΡΑΚΤΗΡΙΣΤΙΚΑ**

4.1 **Ορισμοί Υλικών - Υπηρεσιών**

4.1.1 **Υλικά για Προμήθεια**

4.1.1.1 **Απαιτήσεις ανταλλακτικών για προληπτική συντήρηση 1ου - 2ου κλιμακίου**

4.1.1.1.1 Αναλυτικός Πίνακας απαιτήσεων για τεχνική υποστήριξη σκαφών.

|  |  |  |
| --- | --- | --- |
| **Α/Α** | **Α/Ο ή Ρ/Ν – NCΑGE 88907** | **ΠΕΡΙΓΡΑΦΗ** |
|
|  | 8M0090809 | FILTER |
|  | 8M0000190 | O-RING (4.475 x .210) |
|  | 892584 | SEAL |
|  | 856954 | BUSHING |
|  | 8M0050720 | GASKET |
|  | 8245191 | RETAINER |
|  | 806327 | SCREW (.437-14 x 1.750) |
|  | 889745030 | SCREW (M12 x 30) |
|  | 8M0086290 | CONNECTOR Barb |
|  | 889568001 | ROMMET |
|  | 859731 | FITTING Adapter |
|  | 8M0047424 | TUBING - .25 ID x .48 OD Bulk Cut to 26 inches |
|  | 889792A01 | FITTING KIT Idle Exhaust |
|  | 885527105 | SCREW (M10 x 105) |
|  | 88552785 | SCREW (M10 x 85) |
|  | 8M0102995 | SCREW (M12) \*{ (Long/X-Long)}\* |
|  | 885361A01 | FITTING ASSEMBLY Flush |
|  | 888952 | LINKAGE ARM |
|  | 859578A1 | PLUG ASSEMBLY Oil |
|  | 88552620 | SCREW (M8 x 20) |
|  | 880515 | BOLT (M20 x 68) |
|  | 858951A01 | CLAMP KIT |
|  | 881866 | FITTING |
|  | 8M0047995 | LUG (18 MM) |
|  | 8M0089477 | SEAT Exhaust Seat |
|  | 8M6000694 | RETAINING RING |
|  | 8M0071653 | SCREW Special |
|  | 95084A10 | CABLE ASSEMBLY (5.00 Inches) Red |
|  | 877613A02 | CONNECTOR ASSEMBLY Weather Cap 6 Pin |
|  | 8M0043736 | HOSE |
|  | 8M0022162 | TUD (M10 x 60) |
|  | 8M0099447 | CLIP Connector Mounting |
|  | 897169 | GROMMET |
|  | 8M0047996 | PLUG (24 MM) |
|  | 889846 | FITTING |
|  | 4008850 | SCREW (M6 x 50) |
|  | 858414A04 | CABLE ASSEMBLY Brass Braided |
|  | 8M0082406 | GROMMET Rubber |
|  | 82671117 | NUT (.500-20) |
|  | 8M0034918 | COLLAR |
|  | 8M0045493 | PIN |
|  | 879346T24 | FUSE COVER AND O-RING |
|  | 889540A03 | CLUTCH KIT |
|  | 892445 | O-RING |
|  | 888593 | SEAL Drain Plug |
|  | 8M0053755 | O-ring |
|  | 8M0055058 | TAB WASHER |
|  | 828547T1 | CONDUIT (.500 Inside Diameter x 3.00 Feet Bulk) Cut to 10 inches |
|  | 93388A1 | Decal-Waring-High Voltage |
|  | 896661 | TOOL Fuel Filter |
|  | 897498T07 | EARING Main (White) |
|  | 897498T05 | EARING Main (Green) |
|  | 897498T06 | EARING Main (Navy Blue) |
|  | 897498T08 | EARING Main (Orange) |
|  | 880649002 | LEVER Tilt Lock |
|  | 8M0090010 | WASHER |
|  | 88238T24 | ABLE ASSEMBLY |
|  | 648771 | DIAPHRAGM |
|  | 885518A02 | FITTING ASSEMBLY |
|  | 8M0048079 | LUG 8MM |
|  | 8M0010183 | O-RING |
|  | 8M0088815 | PLUG Panel |
|  | 88552845 | SCREW (M12 x 45) |
|  | 88510940 | SCREW (M14) |
|  | 8M0043519 | ADAPTER |
|  | 899912015 | TAPPET (3.298) |
|  | 899912030 | TAPPET (3.598) |
|  | 899912031 | TAPPET (3.621) |
|  | 899912003 | TAPPET (3.046) |
|  | 899912024 | TAPPET (3.478) |
|  | 899912025 | TAPPET (3.498) |
|  | 889706 | WASHER |
|  | 893394 | KEY With Lock Tab (6.35 mm) |
|  | 8M0027347 | PLUG (M18 x 1.5) |
|  | 899912004 | TAPPET (3.071) |
|  | 899912020 | TAPPET (3.398) |
|  | 899912032 | TAPPET (3.646) |
|  | 899912033 | TAPPET (3.671) |
|  | 899912034 | TAPPET (3.696) |
|  | 899912017 | TAPPET (3.338) |
|  | 899912029 | TAPPET (3.578) |
|  | 893368001 | GROMMET |
|  | 8M0086888 | O-ring |
|  | 887939007 | PLATE Boost Valve Mounting |
|  | 899912002 | TAPPET (3.021) |
|  | 899912035 | TAPPET (3.721) |
|  | 8M0038370 | SCREW (.500-20 x 5.50) |
|  | 899912009 | TAPPET (3.178) |
|  | 899912012 | TAPPET (3.238) |
|  | 899912013 | TAPPET (3.258) |
|  | 899912018 | TAPPET (3.358) |
|  | 899912023 | TAPPET (3.458) |
|  | 899912026 | TAPPET (3.518) |
|  | 95084A13 | CABLE ASSEMBLY (64.00 Inches) |
|  | 899912001 | TAPPET (2.996) |
|  | 899912006 | TAPPET (3.118) |
|  | 899912007 | TAPPET (3.138) |
|  | 899912008 | TAPPET (3.158) |
|  | 899912016 | TAPPET (3.318) |
|  | 899912021 | TAPPET (3.418) |
|  | 899912028 | TAPPET (3.558) |
|  | 899912005 | TAPPET (3.096) |
|  | 899912019 | TAPPET (3.378) |
|  | 888517 | PIN |
|  | 895811155 | SCREW (M10 x 155) |
|  | 8M0103092 | SPRING VALVE KIT Intake and Exhaust |
|  | 899912022 | TAPPET (3.438) |
|  | 896699 | O-RING (1.78 mm x .08 mm) |
|  | 899912010 | TAPPET (3.198) |
|  | 899912011 | TAPPET (3.218) |
|  | 899912014 | TAPPET (3.278) |
|  | 899912027 | TAPPET (3.538) |
|  | 8M0103724 | HARNESS WIF Extension |
|  | 8M0011480 | PLATE Mounting, 14 Pin |
|  | 8M0008031 | Decal-Oil Drain |
|  | 8M0050809 | GROMMET ASSEMBLY |
|  | 892315 | SOUND BLANKET KIT Carbon Edition |
|  | 877769K01 | FILTER Oil (Mercury Branded) |
|  | 816133 | FITTING |
|  | 888958001 | PLUG Flush |
|  | 896842 | SCREW (M6 x 14) |
|  | 889618001 | GASKET Oil Sump |
|  | 8M2003719 | SCREW (M12X1.75X60) |
|  | 8M0105263 | HARNESS WIF Sensor Extension - 36 Inches |
|  | 8M0021532 | SCREW (M12 x 40 MM) \*{ (Left Hand)}\* |
|  | 892335001 | DEFLECTOR Oil |
|  | 8M0043699 | ECAL M-ICON Red, 66mm |
|  | 880629 | SEAL Exhaust Tube |
|  | 826134Q | NODE |
|  | 851889 | O-RING Damper |
|  | 884353 | BRACKET |
|  | 885111 | PIN Dowel (.375 x .875) |
|  | 8855091 | SCREW |
|  | 8M0090182 | Thrust Plate- Long |
|  | 892328T | COVER Helm |
|  | 8172761 | FACEPLATE |
|  | 8M0043703 | M-ICON 66 mm, Black |
|  | 885112 | ASHER |
|  | 888955 | LINK Latch Connecting |
|  | 8M0043266 | SEAL |
|  | 896124 | SLEEVE |
|  | 815504256 | CLAMP Worm Gear |
|  | 79138A8 | CABLE ASSEMBLY (72.00 Inches) Black |
|  | 896951 | PLUG (24 mm) |
|  | 8M0050602 | MAGNET |
|  | 828249 | GROMMET |
|  | 879885Q | FILTER Fuel In-Line |
|  | 8164641 | SEAL Oil |
|  | 896880 | SEAL Valve |
|  | 8M0105264 | HARNESS WIF Sensor Extension - 72 Inches |
|  | 892404A05 | DEFLECTOR ASSEMBLY Water |
|  | 817519A2 | CHECK VALVE ASSEMBLY Drain |
|  | 884462 | SEAL Water |
|  | 8M0117518 | APPLIQUE Starboard, Pearl Fusion |
|  | 893388A01 | CAP Resitor - 2 Pin, 120 Ohm (CAN 1, 2 and 3) |
|  | 889532 | Decal-Trim Relay |
|  | 8M0117520 | APPLIQUE Port, Pearl Fusion |
|  | 8M0080471 | BUMPER Trim |
|  | 88238T23 | CABLE ASSEMBLY |
|  | 892403 | FITTING |
|  | 857137 | SCREW (M12 x 160) \*{ (XX-Long)}\* |
|  | 896966A06 | LONG BLOCK ASSEMBLY |
|  | 8M0053823 | THRUST WASHER |
|  | 8M0033928 | SEAL Oil |
|  | 8M0097716 | DECAL Maintenance 400R |
|  | 8M0064752 | END CAP Cam Tensioner Tensioner |
|  | 8M0032912 | SEAL Top Main Bearing |
|  | 8M0041097 | VALVE KIT Schrader |
|  | 92-858064K01 | SAE 90 Gear Oil (lube) |
|  | 892562T01 | HOUSING Manifold |
|  | 888959 | PIN Hinge |
|  | 888592005 | PLUG ASSEMBLY Oil Drain |
|  | 885094105 | SCREW (M14 x 105) |
|  | 8M0094054 | GASKET Water Passage |
|  | 8M0050692 | BEARING |
|  | 882751A04 | RELAY ASSEMBLY |
|  | 892327 | PLATE Helm Backing \*{ (892557A02)}\* |
|  | 888996 | PRING |
|  | 884325T01 | BEARING ASSEMBLY Roller-Tappered |
|  | 893384001 | COVER Poppet |
|  | 856583A12 | CABLE ASSEMBLY |
|  | 8M0022158 | STUD (M10 x 205) |
|  | 8M0099370 | HOSE ASSEMBLY Supercharger Water Dump |
|  | 895770 | Pin Pivot |
|  | 892005A01 | BEARING Connecting Rod - Blue |
|  | 892005A03 | BEARING Connecting Rod - Orange |
|  | 93388A17 | CABLE ASSEMBLY (8.50 Inches) |
|  | 8M0050688 | WASHER |
|  | 892485003 | PUMP |
|  | 888483 | SEAL Oil |
|  | 8M0088808 | APPLIQUE Port, Warm Fusion |
|  | 8M0095506 | HOSE CAC Tube |
|  | 8M0103481 | DECAL SET Flywheel Cover 350 |
|  | 8M0053734 | O-ring |
|  | 8M0064306 | SPACER |
|  | 8M0010459 | FILLER BLOCK |
|  | 896531090 | SCREW (M16 x 90) |
|  | 8M0050429 | WASHER .030 |
|  | 889633A04 | FITTING ASSEMBLY Flushing |
|  | 8M0103296 | HOSE ASSEMBLY Breather |
|  | 885349501 | SCREW |
|  | 88509530 | SCREW (M8 x 30) |
|  | 8M0034568 | GASKET |
|  | 887938003 | TUBE Rear |
|  | 8M0088807 | APPLIQUE Port, Cold Fusion |
|  | 8M0088809 | APPLIQUE Starboard, Cold Fusion |
|  | 8M0088810 | APPLIQUE Starboard, Warm Fusion |
|  | 889767 | PLUG (12 mm) |
|  | 8M0050425 | WASHER .024 |
|  | 888947501 | DUCT ASSEMBLY Inlet |
|  | 8M0033614 | APPLIQUE Port, Mercury |
|  | 8M0033615 | APPLIQUE Starboard, Mercury |
|  | 897784A01 | BRACKET KIT Upper Chap |
|  | 8M0050430 | WASHER .032 |
|  | 8M0095507 | HOSE CAC Tube |
|  | 891953 | Oil Cooler Housing |
|  | 8M0055652 | TERMINATOR ASSEMBLY 10 Pin (CAN P and H) |
|  | 826709121 | NUT (.625-18) Stainless Steel |
|  | 8M0046569 | RING Thrust |
|  | 8M0053183 | ADAPTER |
|  | 897926 | NUT (M12), Nylon Insert |
|  | 892005A02 | BEARING Connecting Rod - White |
|  | 898908T01 | VALVE Exhaust-Chrome |
|  | 8M0103727 | PARTS MANUAL 350/350 PRO/400R Verado (4-Stroke)(6 Cylinder) |
|  | 8M0007798 | SCREW (M10 x 65) |
|  | 8M0132736 | O-RING KIT |
|  | 898907 | VALVE Intake |
|  | 8M0109756 | DOUBLE NUT KIT Transom Bolt |
|  | 893380 | PIN Clevis |
|  | 887937006 | HOSE |
|  | 8M0039464 | RING Retaining |
|  | 8M0050432 | WASHER .036 |
|  | 8M0050433 | WASHER .038 |
|  | 8M0039993 | FITTING |
|  | 887756 | HOSE Water In-Upper |
|  | 8M0050431 | WASHER .034 |
|  | 8M0087104 | HOSE Hi Pressure Filter |
|  | 8M0090092 | BRACKET FSM Lower |
|  | 8M0046636 | NUT Pinion |
|  | 8M0050438 | WASHER .048 |
|  | 8M0050439 | WASHER .050 |
|  | 892524 | FITTING \*{ (Standard)}\* |
|  | 8M0012083 | ANODE |
|  | 8M0063267 | SHIM SET |
|  | 888930003 | HOSE Cyl Block to IOM |
|  | 889592001 | HOSE |
|  |  | IDLE RELIEF Carbon Edition |
|  | 8M0024870 | ECAL (Mercury Verado) \*{ Air Dam Cap Decal}\* |
|  | 828547753 | CONDUIT (.750 Inside Diameter x 3.00 Feet Bulk) |
|  | 8M0100563 | SEAL ASSEMBLY Rear Cowl, Port and Starboard |
|  | 893404 | ANODE |
|  | 8M0050434 | WASHER .040 |
|  | 8M0096745 | SOUND BLANKET Air Cap |
|  | 8M0092321 | FITTING EDP Black |
|  | 895063001 | INSERT Plastic |
|  | 8M0050437 | WASHER .046 |
|  | 8M0050427 | WASHER .026 |
|  | 8M0050435 | WASHER .042 |
|  | 8M0103480 | DECAL SET Flywheel Cover, 350 Pro |
|  | 8M0063268 | SHIM SET |
|  | 8M0050436 | WASHER .044 |
|  | 76214Q5 | ANODE KIT |
|  | 8M0041096 | FUEL RAIL |
|  | 8M0050428 | WASHER .028 |
|  | 8M4501000 | SCREW (M10 X 342) |
|  | 884330T01 | BEARING ASSEMBLY Tapered |
|  | 8M0010146 | SENSOR \*{ Oil Temperature}\* |
|  | 43585 | COUPLING |
|  | 8M0047129 | COVER ASSEMBLY |
|  | 889246Q39 | SPARK PLUG NGK-ILFR6GE |
|  | 888981001 | HOSE Idle Exhaust |
|  | 888956 | LATCH Hand Lever |
|  | 8M0053505 | TOOL Indicator, Backlash |
|  | 8M0085120 | BRACKET FSM Upper |
|  | 8M0041100 | SCREW (M5 x 10) |
|  | 8M0093150 | OPERATION MANUAL Joystick Piloting |
|  | 8M0041053 | BOOT MAP Sensor |
|  | 8M6000959 | SEAL |
|  | 8M0009261 | BRACKET ASSEMBLY |
|  | 8M0146203 | ELEMENT-FUEL FILT |
|  | 8M0050424 | WASHER .022 |
|  | 8M0053727 | O-ring |
|  | 888971 | RONT LATCH RECEIVER |
|  | 888961A01 | IN ASSEMBLY |
|  | 8M0095659 | FUEL FILTER ASSEMBLY with o-ring, MPP |
|  | 8M0089148 | INSTALLATION MANUAL 400R |
|  | 8M0089145 | INSTALLATION MANUAL Verado L6 |
|  | 8M0089149 | OPERATION MANUAL 400R |
|  | 8M0089146 | OPERATION MANUAL Verado L6 |
|  | 8M0080153 | M-ICON 66 MM Racing |
|  | 880566Q14 | BELT Drive |
|  | 48939A2 | BEARING Tapered Roller |
|  | 889593001 | HOSE |
|  | 888913A01 | POPPET ASSEMBLY |
|  | 8M0046348 | OOL Bearing Driver, Pinion Removal |
|  | 8M0050615 | TOOL Holder, Shift Shaft |
|  | 847635001 | NODE |
|  | 892865 | HOSE Thermostat |
|  | 8M0050423 | WASHER .020 |
|  | 896094A01 | FITTING ASSEMBLY |
|  | 43026Q02 | IMPELLER |
|  | 8806561 | BEARING |
|  | 888461A01 | ITTING KIT |
|  | 855729 | MOUNT |
|  | 8M6002692 | CHAIN Oil Pump Drive Oil Pump Drive |
|  | 8M0008047 | STUD (M12 x 179) \*{ (XX-Long)}\* |
|  | 889727001 | BELL CRANK |
|  | 8M0042697 | HARNESS Fuel Filter Sensor Extension (144 in) |
|  | 895020 | SEAL Manifold Head |
|  | 8M0021043 | SENSOR ASSEMBLY Fuel and Water |
|  | 8M0087122 | HOSE Hi Pressure Filter to Fuel Rail |
|  | 8M0053114 | POOL ASSEMBLY |
|  | 8M0080707 | ENCLOSURE ASSEMBLY -Power Steering Pump |
|  | 895346 | BOLT |
|  | 880624003 | GASKET Block to Adaptor |
|  | 885342002 | SENSOR ASSEMBLY |
|  | 880650003 | SHAFT Tilt Lock |
|  | 880559 | GUIDE Fixed |
|  | 8M0041759 | RACKET Mounting-Starter Motor |
|  | 889675A01 | TOOL Shunt 14-Pin |
|  | 893365T02 | ENCLOSURE ASSEMBLY Top, Power Steering Pump |
|  | 893385001 | RETAINER |
|  | 8M0103362 | CREEN Upper Intake |
|  | 92-8M0078630 | 25W40 4-Cycle, Synthetic Blend Marine Oil 1 Gallon |
|  | 8M0095505 | TUBE CAC |
|  | 8M0087107 | HOSE |
|  | 85978571 | TUBING (52.00 Inches Bulk) To Water Pressure Sensor - Cut to 21.5 Inches |
|  | 8M6002872 | ENSOR ASSEMBLY Knock |
|  | 8M0084506 | HOSE Fuel Inlet Fuel inlet to Fuel Supply Module |
|  | 8M0047428 | HOSE (.25 inch ID, 57.00 Inches Bulk) Cut to 3 inches |
|  | 889617001 | GASKET |
|  | 889552 | FITTING -6 ORB to -6 ORFS (90 Degree) \*{ (Standard)}\* |
|  | 8M0084552 | HOSE Water In Lower |
|  | 881180A02 | RING SET Piston |
|  | 880661 | SEAL |
|  | 8M0055029 | BRACKET Tilt Lock |
|  | 8M0103479 | DECAL SET Flywheel Cover, 400R |
|  | 85944975 | TUBING (72.00 Inches Bulk) Cut to 64 Inches |
|  | 8M0046297 | OIL SEAL ASSEMBLY |
|  | 887753A02 | TUBE ASSEMBLY Oil Drain \*{ (Long)}\* |
|  | 8M0087119 | HOSE Manifold Reference Upper |
|  | 880557 | GUIDE Moveable |
|  | 8M0056639 | RING Retainer |
|  | 88439A25 | CABLE ASSEMBLY Battery - Positive \*{ (Long)}\* |
|  | 8M0046698 | ND CAP ASSEMBLY |
|  | 8M0060041 | FILTER Fuel |
|  | 88439A26 | CABLE ASSEMBLY Battery - Negative \*{ (Long)}\* |
|  | 8M0046557 | HOSE ASSMEBLY Fuel Inlet, 8.2 Inch |
|  | 8M6003035 | ULLEY |
|  | 8M6003465 | VALVE Check |
|  | 8M6003431 | FITTING Water, Supercharger |
|  | 8806621 | BEARING |
|  | 898022 | DIPSTICK Oil |
|  | 884418A1 | TENSIONER ASSEMBLY Oil Pump Drive |
|  | 8M0094053 | PLATE Water Passage |
|  | 899712A01 | CABLE KIT Continuity |
|  | 885541A01 | TUBE ASSEMBLY Water (20.00 Inch) \*{ (Long)}\* |
|  | 8M0082193 | TUBE ASSEMBLY Oil Drain \*{ (X-Long/XX-Long)}\* |
|  | 88535303S | BRACKET |
|  | 8M0046104 | SHIFT SHAFT |
|  | 8M0047448 | TUBING (.312) (70 Inches Bulk) Cut to 21 Inches |
|  | 884323T01 | BEARING ASSEMBLY Roller |
|  | 8M6003432 | FITTING Water, Supercharger |
|  | 8M0026568 | HARNESS ASSEMBLY Signal Driver |
|  | 8M0075217 | DECAL Joystick Piloting \*{ 350}\* |
|  | 8M0046215 | CRANK, Shifter 1/4 Pivot Pin |
|  | 879345T34 | HARNESS ASSEMBLY Trim |
|  | 892967 | HOSE |
|  | 8M0046697 | Thermostat Stop |
|  | 8M0085367 | DECAL 350 HP, Rear |
|  | 885541A03 | TUBE ASSEMBLY Water (30.00 Inch) \*{ (XX-Long)}\* |
|  | 8M0045676 | BEARING Roller |
|  | 885541A02 | TUBE ASSEMBLY Water (25.00 Inch) \*{ (X-Long)}\* |
|  | 8M0032468 | SPACER |
|  | 8M0065258 | BRUSH SET |
|  | 36387A1 | BEARING ASSEMBLY Roller/Cup |
|  | 880550 | SPROCKET Cam Drive |
|  | 895019 | SEAL Manifold to CAC |
|  | 892309T01 | EARING Thrust - Green Crankshaft-Lower |
|  | 892309T04 | EARING Thrust - Navy Blue Crankshaft-Lower |
|  | 884456 | SPROCKET Driven |
|  | 8M0084660 | HOSE Fuel Out Fuel Supply Module |
|  | 87928815T | ISOLATOR |
|  | 8M0046696 | O-RING |
|  | 893409 | TEERING CYLINDER KIT \*{ (Standard)}\* |
|  | 892384T | PLENUM Exhaust |
|  | 8M0089697 | DUCT Inlet |
|  | 8M0053726 | SM TOP HOUSING |
|  | 8M0084774 | HOSE Manifold Reference Lower |
|  | 8M0052590 | TOOL Driver, Upper Driveshaft Bearing |
|  | 8M0011478 | BRACKET Mounting, 14 Pin |
|  | 885363T03 | COVER |
|  | 8M0099017 | DECAL Joystick Piloting, Silver \*{ 400R}\* |
|  | 8M0001491 | NUT Retainer |
|  | 8M0108770 | SCREW (M8X1.25X30) 4 screws per application \*{ Note, screw comes in a pack of 5 pcs.}\* |
|  | 8M0065072 | WATER PUMP REPAIR KIT Upper |
|  | 8M0080491 | CABLE |
|  | 887623T03 | PICKUP ASSEMBLY Oil |
|  | 8M0046360 | TOOL Bearing Driver, Pinion Install |
|  | 898463A01 | TENSIONER ASSEMBLY |
|  | 8M0053116 | SHIM SET |
|  | 8M0057679 | FSM SEAL KIT |
|  | 8M0035594 | TOOL Propeller Shaft Holder |
|  | 8M0047054 | TUBE KIT Fuel Inlet |
|  | 817275A1 | HOUSING KIT Water Pump |
|  | 8M0001734 | ANODE |
|  | 8M4501634 | SOUND BLANKET KIT |
|  | 8M0094213 | HOSE ASSEMBLY Fuel Inlet |
|  | 888416T04 | HARNESS ASSEMBLY DTS, Clean Power, 15 Feet |
|  | 8M0080461 | CABLE Latch |
|  | 893365A03 | Power Steering Pump |
|  | 880805A1 | Screws |
|  | 8M0065064 | SEAL KIT Gearcase |
|  | 8M0063270 | SHIM SET |
|  | 893419 | CAP KIT |
|  | 8M0076286 | SERVICE MANUAL Outboard Joystick Piloting |
|  | 8M0050821 | COVER KIT Flush, Standard |
|  | 897643A01 | HOSE KIT Dampening |
|  | 8M0095674 | BASE ASSEMBLY Fuel Filter |
|  | 8M0082988 | SENSOR Crankshaft Position |
|  | 8M0043229 | SEAL |
|  | 896167A01 | RESERVOIR KIT |
|  | 8M0034048 | VALVE ASSEMBLY Oil Pump |
|  | 8M0046693 | THERMOSTAT ASSEMBLY |
|  | 8M0103287 | Seal |
|  | 896158A01 | RING KIT |
|  | 8M0042300 | SWITCH Trim |
|  | 72957A5 | ANODE ASSEMBLY |
|  | 895854A01 | O-RING KIT |
|  | 896164A01 | TRIM FILTER KIT |
|  | 8M0088927 | HARNESS ASSEMBLY Fuse |
|  | 42600A09 | MERCATHODE ASSEMBLY |
|  | 880615T01 | COIL ASSEMBLY |
|  | 891966006 | BRACKET Cowl \*{ (X-Long/XX-Long)}\* |
|  | 8M0103398 | CHAIN Roller Cam Drive |
|  | 8M0097026 | WEAR PAD |
|  | 8M6000637 | SENSOR Pressure |
|  | 8M0050704 | BEARING Needle |
|  | 8M0011987 | SENSOR \*{ Camshaft Position}\* |
|  | 893364A05 | DECAL, Fluid Type |
|  | 8M0103293 | TUBE ASSEMBLY Hot Air Duct |
|  | 8M0103315 | PITOT SENSOR KIT |
|  | 817275A09 | HOUSING Water Pump-Comple |
|  | 8M0077359 | SEAL |
|  | 8M0001758 | BEARING With Shoulder |
|  | 8M0045604 | SEAL KIT Steering Cylinder |
|  | 8M0062950 | FILTER ASSEMBLY |
|  | 8M0001784 | PIN Rod Eye |
|  | 896160A01 | O-RING KIT |
|  | 8M0103285 | CONNECTING ROD ASSEMBLY |
|  | 896162A01 | TRIM NECK KIT |
|  | 8M0041101 | DAMPER Fuel Rail |
|  | 888974A02 | IDE LATCH ASSEMBLY |
|  | 805382T01 | TOOL Extension-Dial Indicator |
|  | 889656T01 | HROUD |
|  | 893408A01 | PIN KIT Trim |
|  | 8M0103295 | INTAKE ASSEMLY Duct |
|  | 896159A01 | PISTON KIT |
|  | 8M0119299 | COVER Chaps, Front, Pearl Fusion |
|  | 8M0053113 | CLUTCH |
|  | 8M0103375 | OUNT CRADLE \*{ 350 Models only}\* |
|  | 8M0110315 | LATE Retainer |
|  | 809905001 | WRENCH Torque Adapter |
|  | 8M0053749 | O-ring |
|  | 8M0089147 | SERVICE MANUAL Verado L6 |
|  | 8M0105203 | TOOL TRIM CYLINDER END CAP |
|  | 8M0100565 | COVER Chaps, Front, Warm Fusion |
|  | 892864T04 | THERMOSTAT ASSEMBLY |
|  | S-1200-RF01 | Roll Bar |
|  | S-1200-GN01 | Βάση όπλου 0.50 |
|  | S-1200-GN02 | Βάση όπλου 7,62 |
|  | RΜ-916-001 | Φανάρι κόκκινο θέσεως με φλας |
|  | RΜ-916-002 | Φις μεταλλικό, 7 PIN, αρσενικό |
|  | RΜ-916-003 | Εργάτης τρέιλερ βαρέως τύπου 4000lb |
|  | RΜ-916-004 | Πόδι τρέιλερ ρυθμιζόμενο με μεταλλική ζάντα και συμπαγή ρόδα |
|  | RΜ-916-005 | Ιμάντας πολυεστερικός με γάντζο γαλβανιζέ |
|  | RΜ-916-006 | Ράουλα καρίνας και πλώρης |
|  | RΜ-916-007 | Ράουλο τρέιλερ πλευρικό |
|  | RΜ-916-008 | Ελαστικό 185R14 |
|  | 0092-858084-QE1 | ΛΑΔΙ 4-STR 25W50 HP VERADO 4L |
|  | 0092-8M0096-256 | ΛΑΔΙ 4-STR 25W50 HP SYNTHETIC 1L |
|  | 0035-879885-Q | ΦΙΛΤΡΟ ΒΕΝΖΙΝΗΣ |
|  | 0092-8M0079-744 | ΚΑΘΑΡΙΣΤΙΚΟ ΒΕΝΖΙΝΗΣ QUICKLEEN |
|  | 0000-8934404 | ΑΝΟΔΙΟ |
|  | 0000-826134-Q | ΑΝΟΔΙΟ |
|  | 0000-076214-Q5 | ΑΝΟΔΙΟ |
|  | 0092-8M0208-465 | ΓΡΑΣΣΟ ΘΑΛΑΣΣΗΣ 2-4-C 240ml |
|  | 0092-8M0184-794 | ΑΝΤΙΣΚΩΡΙΑΚΟ ΣΠΡΕΥ 360ml |
|  | 0047-043026-Q02 | ΦΤΕΡΩΤΗ |
|  | 0092-8M0219-575 | ΒΑΛΒΟΛΙΝΗ HP 1L |
|  | 0097-8M0217-563 | ΑΝΟΔΙΟ |
|  | 0000-8M0120-657 | ΚΙΤ ΣΕΡΒΙΣ 100ΩΡΩΝ L6 VERADO GEN V |
|  | 00008M0217-561 | ΑΝ0ΔΙΟ |
|  | 0035-8777769-Q01 | ΦΙΛΤΡΟ ΛΑΔΙΟΥ |
|  | 0092-802854-Q1 | ΒΑΛΒΟΛΙΝΗ HP 1 L |
|  | 0035-8M0090-809 | ΦΙΛΤΡΟ ΒΕΝΖΙΝΗΣ |
|  | 0026-888593- | ΤΣΙΜΟΥΧΑ ΤΑΠΑ ΛΑΔΙΟΥ |
|  | 0026-830749- | ΤΣΙΜΟΥΧΑ ΤΑΠΑΣ ΒΑΛΒΟΛΙΝΗΣ |
|  | 0000-817275-Α09 | ΑΝΤΛΙΑ ΝΕΡΟΥ ΠΛΗΡΗΣ |
|  | 0033-889246-Q39 | ΜΠΟΥΖΙ ILFR6GE |
|  | 0000-892864-T04 | ΘΕΡΜΟΣΤΑΤΗΣ |
|  | 0057-880566-Q14 | ΙΜΑΝΤΑΣ |
|  | 0057-880566-Q1 | ΑΝΟΔΙΟ |
|  | 0000-893404- | ΑΝΟΔΙΟ |

4.1.1.1.2 Αναλυτικός Πίνακας απαιτήσεων για τεχνική υποστήριξη των εξωλέμβιων κινητήρων Mercury 5.7 L V10 400hp Verado XL»

|  |  |  |
| --- | --- | --- |
| **α/α** | **Α/Ο ή Ρ/Ν – NCΑGE 88907** | **ΠΕΡΙΓΡΑΦΗ** |
| 1 | 8Μ0205848 | ΦΙΛΤΡΟ ΛΑΔΙΟΥ |
| 2 | 0092-8M0086-227 | ΛΑΔΙ 4-STR 25W40 HP VERADO 4L |
| 3 | 0092-8Μ0133995 | ΒΑΛΒΟΛΙΝΗ HP 1 L |
| 4 | 0097-8M0207-809 | ΣΕΤ ΑΝΟΔΙΑ V10 |
| 5 | 0000-8M0207-807 | ΚΙΤ ΣΕΡΒΙΣ 100 ΩΡΩΝ V10 |
| 6 | 8M0200115 | ΦΤΕΡΩΤΗ |
| 7 | S1200-01 | ΣΕΤ ΑΝΟΔΙΑ ΣΚΑΦΟΥΣ |
| 8 | S1200-02 | ΦΙΛΤΡΟ ΥΔΑΤΟΠΑΓΙΔΑΣ |
| 9 | 0047-8M0200-115 | ΦΤΕΡΩΤΗ V10 |
| 10 | 1056105/6 NCAGE: R1172 | ΚΥΤΙΟ ΠΡΩΤΩΝ ΒΟΗΘΕΙΩΝ |
| 11 | 1000313 NCAGE: R1172 | ΚΥΤΙΟ ΝΕΡΟΥ |
| 12 | 1000315 NCAGE: R1172 | ΚΥΤΙΟ ΤΡΟΦΗΣ |
| 13 | 7668Ε NCAGE: H1G03 | Μουράβια Hempel Hard Racing (λίτρα) |

4.1.1.2 **Απαιτήσεις ανταλλακτικών για συντήρηση 3ου κλιμακίου**.

4.1.1.2.1 Αναλυτικός Πίνακας απαιτήσεων για τεχνική υποστήριξη σκαφών.

|  |  |  |
| --- | --- | --- |
| **Α/Α** | **Α/Ο ή Ρ/Ν – NCΑGE 88907** | **ΠΕΡΙΓΡΑΦΗ** |
|
| 1. 1 | 8M0047949 | SHIFT SHAFT |
| 1. 2 | 8M6000639 | SENSOR Pressure |
| 1. 3 | 885561T | OVER Fuse Box |
| 1. 4 | 8M0001803 | Decal-Serial Overlaminate |
| 1. 5 | 8M0103686 | FUEL FILTER KIT Engine Mounted Optional |
| 1. 6 | 893420A01 | MANUAL RELEASE KIT |
| 1. 7 | 8M0078858 | WATER PUMP REPAIR KIT Complete |
| 1. 8 | 8M0078614 | WRENCH Power Steering Cylinder End Cap Spanner |
| 1. 9 | 809463A1 | SOLENOID KIT |
| 1. 10 | 889283A01 | TOOL KIT Fuel Priming |
| 1. 11 | 8M6002465 | INJECTOR ASSEMBLY Fuel |
| 1. 12 | 880639T | SUMP ASSEMBLY Oil |
| 1. 13 | 893405T | COVER |
| 1. 14 | 8M0102452 | MOUNT Front |
| 1. 15 | 881879T26 | SENSOR Pressure Water |
| 1. 16 | 891663001 | SENSOR ASSEMBLY Temperature |
| 1. 17 | 8M0010626 | SENSOR Trim Position-Black |
| 1. 18 | 8M0095669 | FUEL FILTER KIT with o-ring, MPP Remote Mounted |
| 1. 19 | 8M0096287 | DECAL KIT 400R Racing |
| 1. 20 | 885560T03 | Electrical Box-Complete |
| 1. 21 | 8M0050726 | COVER KIT |
| 1. 22 | 72958A5 | ELECTRODE ASSEMBLY |
| 1. 23 | 8M0100564 | COVER Chaps, Front, Cold Fusion |
| 1. 24 | 896163A01 | PUMP KIT Trim |
| 1. 25 | 8M0080961 | TUBE ASSEMBLY Exhaust |
| 1. 26 | 8M0048178 | SHAFT Shift (Long) |
| 1. 27 | 8M4501639 | SOUND BLANKET KIT |
| 1. 28 | 8M0105447 | PAD Wear |
| 1. 29 | 8M0046632 | TOOL Holder, Pinion Nut |
| 1. 30 | 88334A2 | MERCATHODE KIT |
|  | 8M0101707 | ELT TENSIONER |
|  | 8M0119293 | AP, Air Dam Pearl Fusion |
|  | 895374T | GASKET Head |
|  | 896165A01 | Manifold Kit, Trim |
|  | 8M0100173 | FRONT COWL ASSEMBLY Port and Starboard, Cold Fusion |
|  | 8M0100172 | FRONT COWL ASSEMBLY Port and Starboard, Mercury |
|  | 8M0119301 | FRONT COWL ASSEMBLY Port and Starboard, Pearl Fusion |
|  | 8M0100174 | FRONT COWL ASSEMBLY Port and Starboard, Warm Fusion |
|  | 8M0103283 | CAP |
|  | 884446T04 | PUMP ASSEMBLY Oil |
|  | 896157A01 | RIM ROD KIT \*{ [2B368739] & Below}\* |
|  | 8M0118299 | RIM ROD KIT \*{ [2B368740] & Up}\* |
|  | 8M0103291 | INTAKE ASSEMBLY Lower |
|  | 880552A07 | GASKET SET Powerhead |
|  | 884458T07 | DRIVESHAFT Oil Pump |
|  | 8M0102448 | DECAL SET Mercury |
|  | 888976T01 | BRACKET |
|  | 8M0071622 | SPACER Driveshaft Housing X-Long Black \*{ (XX-Long)}\* |
|  | 880665T01 | ARM Steering |
|  | 8M0104286 | PISTON ASSEMBLY |
|  | 8M0103289 | PUMP ASSEMBLY Low Pressur |
|  | 8M0076745 | SHIM SET |
|  | 888983T03 | LYWHEEL ASSEMBLY |
|  | 892596T04 | COVER ASSEMBLY Cam |
|  | 8M0100196 | SPACER Driveshaft Housing X-Long Silver \*{ (XX-Long)}\* |
|  | 8M0103288 | PUMP ASSEMBLY High Pressure |
|  | 895343T02 | TOOL Flywheel Puller |
|  | 8M0083678 | MANIFOLD ASSEMBLY Intake |
|  | 885354T01 | AP, Air Dam Mercury, Black |
|  | 8M0103301 | SHAFT Drive, Long |
|  | 8M0103043 | DECAL 350 Pro, Top |
|  | 8M0103311 | BRACKET ASSEMBLY Front Mount |
|  | 8M0100547 | LATCH ASSEMBLY Front and Side |
|  | 8M0090475 | AP, Air Dam Warm Fusion |
|  | 8M0103042 | DECAL SET ME Verado Racing, Black (Does Not Contain Carbon Decals) |
|  | 892339T01 | STARTER MOTOR ASSEMBLY |
|  | 8M0046694 | O-RING |
|  | 8M0103284 | CAMSHAFT Exhaust |
|  | 8M0053124 | GEAR KIT Reverse \*{ 1.75:1 Ratio}\* |
|  | 8M0090474 | AP, Air Dam Cold Fusion |
|  | 892557T01 | HELM Standard (32 cc) |
|  | 880552A08 | GASKET SET Powerhead |
|  | 892380T01 | HELM Standard (40 cc) |
|  | 8M0053120 | GEAR SET 12/21 (1.75:1) Forward |
|  | 892940T02 | ALTERNATOR |
|  | 892380A02 | STEERING HELM KIT Standard (40 cc) |
|  | 8M0053121 | GEAR KIT Reverse \*{ 1.75:1 Ratio}\* |
|  | 892558T01 | HELM Standard (50 cc) |
|  | 8M0103303 | SHAFT Drive, X-Long |
|  | 892558A02 | STEERING HELM KIT Standard (50 cc) |
|  | 896156A01 | TRIM CYLINDER KIT |
|  | 8M0118298 | TRIM CYLINDER KIT \*{ [2B368740] & Up}\* |
|  | 8M0103304 | SHAFT Drive, XX-Long |
|  | 8M0078258 | GEAR SET 12/21(1.75:1) Forward and Pinion \*{ Standard Rotation}\* |
|  | 8M0102451 | COVER Flywheel |
|  | 892557A02 | STEERING HELM KIT Standard (32 cc) |
|  | 0048-857029-A46 | Revolution Propeller L |
|  | 0048-857028-A46 | Revolution Propeller R |
|  | 8M0103041 | ECAL SET ME Verado Pro |
|  | 896161A02 | TRIM MOTOR KIT |
|  | 822778004 | TOOL Adaptor Fitting-Power Trim |
|  | 8M0046443 | OOL Height Gageing, pinion |
|  | 884408A08 | VALVE KIT Control - Electric Boost |
|  | 8M0100556 | CHAPS ASSEMBLY Long, Port and Starboard, Black |
|  | 8M0103333 | PLATES ASSEMBLY Thrust, X-Long |
|  | 8M0103297 | HOUSING Driveshaft Long, Black |
|  | 8M0103294 | HOUSING Driveshaft Long, Silver |
|  | 8M0103300 | PROPELLER SHAFT 1.25 Inch \*{ 1.75:1 Ratio}\* |
|  | 8M0103298 | HOUSING Driveshaft X-Long, Black |
|  | 8M0103302 | CARRIER ASSEMBLY Bearing |
|  | 8M0100560 | CHAPS ASSEMBLY X-Long, Port and Starboard, Black |
|  | 8M0103305 | CARRIER ASSEMBLY Bearing |
|  | 8M0119296 | CHAPS ASSEMBLY X-Long, Port and Starboard, Pearl Fusion |
|  | 8M0119298 | CHAPS ASSEMBLY Long, Port and Starboard, Pearl Fusion |
|  | 8M0100559 | CHAPS ASSEMBLY Long, Port and Starboard, Warm Fusion |
|  | 892126A03 | ADAPTER PLATE KIT |
|  | 8M0100558 | CHAPS ASSEMBLY Long, Port and Starboard, Cold Fusion |
|  | 8M0102455 | MODULE Fuel Supply |
|  | 8M0085008 | FUEL RAIL ASSEMBLY |
|  | 888991T04 | CONTROL ASSEMBLY Throttle - Electronic |
|  | 8M0103332 | PLATES ASSEMBLY Thrust, Long |
|  | 8M0100561 | CHAPS ASSEMBLY X-Long, Port and Starboard, Cold Fusion |
|  | 8M0100562 | CHAPS ASSEMBLY X-Long, Port and Starboard, Warm Fusion |
|  | 8M0119302 | REAR COWL ASSEMBLY Pearl Fusion, Non-Decaled |
|  | 8M0103306 | HOUSING Driveshaft X-Long, Silver |
|  | 8M0102454 | HARNESS ASSEMBLY Engine |
|  | 8M0110314 | MOUNTING PLATE |
|  | 880652T02 | Transom Assembly |
|  | 8M0103373 | HEAD Steering |
|  | 880660T02 | TUBE Steering |
|  | 8M0080200 | PUMP KIT Power Steering (12 Feet) |
|  | 8M0080201 | PUMP KIT Power Steering (24 Feet) |
|  | 8M0080199 | PUMP KIT Power Steering (4 Feet) |
|  | 8M0119289 | TOP COWL ASSEMBLY Pearl Fusion, Non-Decaled |
|  | 8M0100176 | REAR COWL ASSEMBLY Cold Fusion, Non-Decaled |
|  | 8M0100221 | TOP COWL ASSEMBLY Cold Fusion, Non-Decaled |
|  | 8M0100177 | REAR COWL ASSEMBLY Warm Fusion, Non-Decaled |
|  | 8M0110312 | MOUNT ASSEMBLY Rear Port |
|  | 8M0110313 | MOUNT ASSEMBLY Rear Starboard |
|  | S-EL-010 / NCAGE U4671 | SIMRAD NSSevo3 12-inch display with GPS, sounder & Wi-Fi. |
|  | S-EL-011 / NCAGE U4671 | Simrad HALO20+ 36 NM 20-inch pulse compression radar, 60 RPM, VelocityTrack™,Dual Range. |
|  | S-EL-012 / NCAGE U4671 | The Precision-9 Compass. Outputs Heading (20Hz), Rate Of Turn (20 Hz), roll, and pitch (10 hZ) over the NMEA 2000® network. |
|  | S-EL-013 / NCAGE U4671 | NAIS-500 + NSPL500 kit. Includes GPS500 antenna and 1.8 m (6ft) Micro-C cable and T connector. |
| 1. 140 | S-EL-014 / NCAGE U4671 | Simrad RS20S Class D DSC VHF Radio: Entry level VHF radio with NMEA2000 connectivity for GPS position. |
| 1. 141 | S-EL-015 / NCAGE U4671 | NMEA 2000 Micro-C Network starter kit: Includes Network power cable, 4.5 m (15 ft) N2K cable, 3 x T-connectors, 2 x network terminators |
| 1. 142 | S-EL-016 / NCAGE U4671 | N2KEXT-6RD - 1.82 m (6-ft) NMEA 2000 |
| 1. 143 | S-EL-017 / NCAGE U4671 | Navionics 43XG - Mediterranean Sea & Black Sea - SD Card 43XG/MSD |
| 1. 144 | S-EL-018 / NCAGE U4671 | Navico 1720 VHF antenna, 1.1 m (3 ft) stainless |
| 1. 145 | S-EL-200 / G2680 | Προβολέας έρευνας τύπου LED 200.000 κεριά τηλεχειριζόμενος |
| 1. 146 | S-EL-300 / G2769 | Αναλαμπών κυανός φάρος τύπου LED 10 μοτίβων JULUEN B16 |
| 1. 147 | SW-S2-1300 / G2680 | S2 Shockwave Shockabsorbing Pilot Seats |
| 1. 148 | S-1200-SSJ-2400 / G2680 | Jockey Seats |
| 1. 149 | S-1200-FS2M/ G2680 | Fender 2 m per piece |
| 1. 150 | S-1200-FIC/ G2680 | Fender Inner Cover |
| 1. 151 | S-1200-FOC / G2680 | Fender Outercover |
| 1. 152 | S-1200-SSFT-380 / G2680 | Fuel tank 380lts |
| 1. 153 | RΜ-916-009 / G2680 | Άξονας Τρέιλερ 2500 Kg με Φρένο & Στεγανά Ρουλεμάν Βαλβολίνης |
| 1. 154 | RΜ-916-010/ G2680 | Δακτύλιος φρένου αδράνειας |
| 1. 155 | RΜ-916-011/ G2680 | Μηχανισμός φρένου αδρανείας |
| 1. 156 | RΜ-916-012/ G2680 | Γράσο τροχών τρέϊλερ 1kg |
| 1. 157 | RΜ-916-013/ G2680 | Ρουλεμάν τροχού τρέϊλερ |
| 1. 158 | 0000-S-1200-T/ G2680 | Φορέας Τρέιλερ Roadmaster |
| 1. 159 | TM-100-112 | Εγχειρίδια συντήρησης εξωλέμβιας μηχανής MERCURY VERADO 400Hp 3ου Κλιμ |
| 1. 160 | TM-100-113 | Εγχειρίδιο συντήρησης Simrad GO9 XSE - Simrad Halo 24-VHF RS40 3ου κλιμ |
| 1. 161 | TM-100-114 | Εγχειρίδιο συντήρησης ταχύπλοου σκάφους "MUNIN 1200" 3ου Κλιμ |
| 1. 162 | 0057-880566-Q14 | ΙΜΑΝΤΑΣ |
| 1. 163 | 0000-8Μ0078-858 | ΣΕΤ ΑΝΤΛΙΑΣ ΝΕΡΟΥ |
| 1. 164 | 0000-8Μ0174-561 | ΘΕΡΜΟΣΤΑΤΗΣ |
| 1. 165 | 0033-8M0176-653 | ΜΠΟΥΖΙ ILFTR6GE |
| 1. 166 | 0097-8M0217-563 | ΑΝΟΔΙΟ |
| 1. 167 | 0000-8M0097-858 | ΚΙΤ ΣΕΡΒΙΣ 300ΩΡΩΝ L6 VERADO GEN V |

4.1.1.2.2 Αναλυτικός Πίνακας απαιτήσεων για τεχνική υποστήριξη των εξωλέμβιων κινητήρων Mercury 5.7 L V10 400hp Verado XL»

|  |  |  |
| --- | --- | --- |
| **α/α** | **Α/Ο ή Ρ/Ν – NCΑGE 88907** | **ΠΕΡΙΓΡΑΦΗ** |
|  | 0092-8M0086-226 | ΛΑΔΙ 4-STR 25W40 SYNTHETIC 1L |
|  | 0092-8M0133-995 | ΒΑΛΒΟΛΙΝΗ HP 1 L RAC |
|  | 0000-8M0207-808 | ΚΙΤ ΣΕΡΒΙΣ 300 ΩΡΩΝ V10 |
|  | 0092-8M0133-951 | ΛΑΔΙ ΤΙΜΟΝΙΟΥ VERADO 1L |
|  | 0092-858075-QB1 | ΛΑΔΙ ΥΔΡΑΥΛΙΚΩΝ ΣΥΣΤΗΜΑΤΩΝ 1L |
|  | 26-888593- | ΤΣΙΜΟΥΧΑ ΤΑΠΑ ΛΑΔΙΟΥ |
|  | 8Μ0204693 | ΤΣΙΜΟΥΧΑ ΤΑΠΑΣ ΒΑΛΒΟΛΙΝΗΣ |
|  | 0092-858076/Κ01 | Λάδι Τιμονιού VERADO (λίτρο) |
|  | S1200-03 NCΑGE: Y.ΕΚΔ | Ρουλεμαν Κίτ Επ. LM67048/25580 |
|  | S1200-04 NCΑGE: Y.ΕΚΔ | Σετ ακροδεκτών S1200 |

|  |  |
| --- | --- |
| ΕΓΚΡΙΣΗ  ΤΕΧΝΙΚΗΣ ΠΡΟΔΙΑΓΡΑΦΗΣ  ΠΕΔ -Α-  ΕΚΔΟΣΗ 2η  ΤΡΟΠΟΠΟΙΗΣΗ 1η | |
| ΣΥΝΤΑΞΗ | Δημήτριος Ζησίμου  Ταγματάρχης (ΠΖ) |
| ΕΛΕΓΧΟΣ |  |
| ΘΕΩΡΗΣΗ | Χρήστος Σπανίδης  Ταξίαρχος  ΙΟΥΝΙΟΣ 2025 |